| ### Showing:
Annotations
Attributes
Diagrams
Instances
Model
Properties
Source
Used by

Element cr:HandsetDeviceType / cr:handsetMake

Namespace | urn:CellexReport
Annotations | Company that manufactured handset.
Diagram |
Type | xs:string
Properties |
content | simple
minOccurs | 0
Source |
    <xs:element name="handsetMake" type="xs:string" minOccurs="0">
      <xs:annotation>
        <xs:documentation>Company that manufactured handset.</xs:documentation>
      </xs:annotation>
    </xs:element>
Schema location | CellexReport.xsd Copy and paste this link to your file browser, clicking the link MAY open in the browser. Opening in an XML aware editor is best.

Element cr:HandsetDeviceType / cr:handsetModel

Namespace | urn:CellexReport
Annotations | Model number of handset
Diagram |
Type | xs:string
Properties |
content | simple
minOccurs | 0
Source |
    <xs:element name="handsetModel" type="xs:string" minOccurs="0">
      <xs:annotation>
        <xs:documentation>Model number of handset</xs:documentation>
      </xs:annotation>
    </xs:element>
Schema location | CellexReport.xsd Copy and paste this link to your file browser, clicking the link MAY open in the browser. Opening in an XML aware editor is best.

Element cr:HandsetDeviceType / cr:imei

Namespace | urn:CellexReport
Annotations | International Mobile Equipment Identity or IMEI is a number (decimal), usually unique to identify GSM, WCDMA, and iDEN mobile phones, as well as some satellite phones. It is usually found printed inside the battery compartment of the phone. It can also be displayed on the screen of the phone by entering *#06# into the keypad on most phones.
Diagram |
Type | xs:string
Properties |
content | simple
minOccurs | 0
Source |
    <xs:element name="imei" type="xs:string" minOccurs="0">
      <xs:annotation>
        <xs:documentation>International Mobile Equipment Identity or IMEI is a number (decimal), usually unique to identify GSM, WCDMA, and iDEN mobile phones, as well as some satellite phones. It is usually found printed inside the battery compartment of the phone. It can also be displayed on the screen of the phone by entering *#06# into the keypad on most phones.</xs:documentation>
      </xs:annotation>
    </xs:element>
Schema location | CellexReport.xsd Copy and paste this link to your file browser, clicking the link MAY open in the browser. Opening in an XML aware editor is best.

Element cr:HandsetDeviceType / cr:hardwareVersion

Namespace | urn:CellexReport
Annotations | Refers to the version of the hardware of a handset or a CELLEX kit.
Diagram |
Type | xs:string
Properties |
content | simple
minOccurs | 0
Source |
    <xs:element name="hardwareVersion" type="xs:string" minOccurs="0">
      <xs:annotation>
        <xs:documentation>Refers to the version of the hardware of a handset or a CELLEX kit.</xs:documentation>
      </xs:annotation>
    </xs:element>
Schema location | CellexReport.xsd Copy and paste this link to your file browser, clicking the link MAY open in the browser. Opening in an XML aware editor is best.

Element cr:HandsetDeviceType / cr:softwareVersion

Namespace | urn:CellexReport
Annotations | Refers to the software version of a handset.
Diagram |
Type | xs:string
Properties |
content | simple
minOccurs | 0
Source |
    <xs:element name="softwareVersion" type="xs:string" minOccurs="0">
      <xs:annotation>
        <xs:documentation>Refers to the software version of a handset.</xs:documentation>
      </xs:annotation>
    </xs:element>
Schema location | CellexReport.xsd Copy and paste this link to your file browser, clicking the link MAY open in the browser. Opening in an XML aware editor is best.

Element cr:HandsetDeviceType / cr:timeSetTo

Namespace | urn:CellexReport
Annotations | Refers to the time that the handset was set once the phone was exploited. Most of the time it will be the same as Actual Time, but there have been cases where phones were not in sync with the real time.
Diagram |
Type | cr:NormalizedDateTimeType
Properties |
content | complex
minOccurs | 0
Attributes |
QName | Type | Use |
--- | --- | --- | ---
normalizedDate | xs:date | optional |
normalizedDateTime | xs:dateTime | optional |
rawDateTime | xs:string | required |
Source |
    <xs:element name="timeSetTo" type="cr:NormalizedDateTimeType" minOccurs="0">
      <xs:annotation>
        <xs:documentation>Refers to the time that the handset was set once the phone was exploited. Most of the time it will be the same as Actual Time, but there have been cases where phones were not in sync with the real time.</xs:documentation>
      </xs:annotation>
    </xs:element>
Schema location | CellexReport.xsd Copy and paste this link to your file browser, clicking the link MAY open in the browser. Opening in an XML aware editor is best.

Element cr:HandsetDeviceType / cr:actualTime

Namespace | urn:CellexReport
Annotations | The actual time when the handset is exploited by a CELLEX kit.
Diagram |
Type | cr:NormalizedDateTimeType
Properties |
content | complex
minOccurs | 0
Attributes |
QName | Type | Use |
--- | --- | --- | ---
normalizedDate | xs:date | optional |
normalizedDateTime | xs:dateTime | optional |
rawDateTime | xs:string | required |
Source |
    <xs:element name="actualTime" type="cr:NormalizedDateTimeType" minOccurs="0">
      <xs:annotation>
        <xs:documentation>The actual time when the handset is exploited by a CELLEX kit.</xs:documentation>
      </xs:annotation>
    </xs:element>
Schema location | CellexReport.xsd Copy and paste this link to your file browser, clicking the link MAY open in the browser. Opening in an XML aware editor is best.

Element cr:HandsetDeviceType / cr:memoryCards

Namespace | urn:CellexReport
Diagram |
Properties |
content | complex
minOccurs | 0
Model | cr:memoryCard+
Children | cr:memoryCard
Instance |
    <cr:memoryCards xmlns:cr="urn:CellexReport">
      <cr:memoryCard>{1,unbounded}</cr:memoryCard>
    </cr:memoryCards>
Source |
    <xs:element name="memoryCards" minOccurs="0">
      <xs:complexType>
        <xs:sequence>
          <xs:element name="memoryCard" type="xs:string" maxOccurs="unbounded">
            <xs:annotation>
              <xs:documentation>Refers to whether a phone has a memory card within it during capture. Typical memory cards are SD cards.</xs:documentation>
            </xs:annotation>
          </xs:element>
        </xs:sequence>
      </xs:complexType>
    </xs:element>
Schema location | CellexReport.xsd Copy and paste this link to your file browser, clicking the link MAY open in the browser. Opening in an XML aware editor is best.

Element cr:HandsetDeviceType / cr:memoryCards / cr:memoryCard

Namespace | urn:CellexReport
Annotations | Refers to whether a phone has a memory card within it during capture. Typical memory cards are SD cards.
Diagram |
Type | xs:string
Properties |
content | simple
maxOccurs | unbounded
Source |
    <xs:element name="memoryCard" type="xs:string" maxOccurs="unbounded">
      <xs:annotation>
        <xs:documentation>Refers to whether a phone has a memory card within it during capture. Typical memory cards are SD cards.</xs:documentation>
      </xs:annotation>
    </xs:element>
Schema location | CellexReport.xsd Copy and paste this link to your file browser, clicking the link MAY open in the browser. Opening in an XML aware editor is best.

Element cr:HandsetDeviceType / cr:greetingMessage

Namespace | urn:CellexReport
Annotations | Refers to a possible message on a handset, which is displayed once the handset is turned on.
Diagram |
Type | xs:string
Properties |
content | simple
minOccurs | 0
Source |
    <xs:element name="greetingMessage" type="xs:string" minOccurs="0">
      <xs:annotation>
        <xs:documentation>Refers to a possible message on a handset, which is displayed once the handset is turned on.</xs:documentation>
      </xs:annotation>
    </xs:element>
Schema location | CellexReport.xsd Copy and paste this link to your file browser, clicking the link MAY open in the browser. Opening in an XML aware editor is best.

Element cr:HandsetDeviceType / cr:keypadLockCode

Namespace | urn:CellexReport
Annotations | The code to unlock a locked phone. Typically a 4 digit number.
Diagram |
Type | xs:string
Properties |
content | simple
minOccurs | 0
Source |
    <xs:element name="keypadLockCode" type="xs:string" minOccurs="0">
      <xs:annotation>
        <xs:documentation>The code to unlock a locked phone. Typically a 4 digit number.</xs:documentation>
      </xs:annotation>
    </xs:element>
Schema location | CellexReport.xsd Copy and paste this link to your file browser, clicking the link MAY open in the browser. Opening in an XML aware editor is best.

Element cr:HandsetDeviceType / cr:bluetoothID

Namespace | urn:CellexReport
Annotations | The unique 48-bit address of the Bluetooth device.
Diagram |
Type | xs:string
Properties |
content | simple
minOccurs | 0
Source |
    <xs:element name="bluetoothID" type="xs:string" minOccurs="0">
      <xs:annotation>
        <xs:documentation>The unique 48-bit address of the Bluetooth device.</xs:documentation>
      </xs:annotation>
    </xs:element>
Schema location | CellexReport.xsd Copy and paste this link to your file browser, clicking the link MAY open in the browser. Opening in an XML aware editor is best.

Complex Type cr:HandsetDeviceType

Namespace | urn:CellexReport
Diagram |
Used by |
Element | cr:CellexReportDataType/cr:handsetInfo
Model | ALL( cr:handsetMake{0,1} cr:handsetModel{0,1} cr:imei{0,1} cr:hardwareVersion{0,1} cr:softwareVersion{0,1} cr:timeSetTo{0,1} cr:actualTime{0,1} cr:memoryCards{0,1} cr:greetingMessage{0,1} cr:keypadLockCode{0,1} cr:bluetoothID{0,1} )
Children | cr:actualTime , cr:bluetoothID , cr:greetingMessage , cr:handsetMake , cr:handsetModel , cr:hardwareVersion , cr:imei , cr:keypadLockCode , cr:memoryCards , cr:softwareVersion , cr:timeSetTo
Source |
    <xs:complexType name="HandsetDeviceType">
      <xs:all>
        <xs:element name="handsetMake" type="xs:string" minOccurs="0">
          <xs:annotation>
            <xs:documentation>Company that manufactured handset.</xs:documentation>
          </xs:annotation>
        </xs:element>
        <xs:element name="handsetModel" type="xs:string" minOccurs="0">
          <xs:annotation>
            <xs:documentation>Model number of handset</xs:documentation>
          </xs:annotation>
        </xs:element>
        <xs:element name="imei" type="xs:string" minOccurs="0">
          <xs:annotation>
            <xs:documentation>International Mobile Equipment Identity or IMEI is a number (decimal), usually unique to identify GSM, WCDMA, and iDEN mobile phones, as well as some satellite phones. It is usually found printed inside the battery compartment of the phone. It can also be displayed on the screen of the phone by entering *#06# into the keypad on most phones.</xs:documentation>
          </xs:annotation>
        </xs:element>
        <xs:element name="hardwareVersion" type="xs:string" minOccurs="0">
          <xs:annotation>
            <xs:documentation>Refers to the version of the hardware of a handset or a CELLEX kit.</xs:documentation>
          </xs:annotation>
        </xs:element>
        <xs:element name="softwareVersion" type="xs:string" minOccurs="0">
          <xs:annotation>
            <xs:documentation>Refers to the software version of a handset.</xs:documentation>
          </xs:annotation>
        </xs:element>
        <xs:element name="timeSetTo" type="cr:NormalizedDateTimeType" minOccurs="0">
          <xs:annotation>
            <xs:documentation>Refers to the time that the handset was set once the phone was exploited. Most of the time it will be the same as Actual Time, but there have been cases where phones were not in sync with the real time.</xs:documentation>
          </xs:annotation>
        </xs:element>
        <xs:element name="actualTime" type="cr:NormalizedDateTimeType" minOccurs="0">
          <xs:annotation>
            <xs:documentation>The actual time when the handset is exploited by a CELLEX kit.</xs:documentation>
          </xs:annotation>
        </xs:element>
        <xs:element name="memoryCards" minOccurs="0">
          <xs:complexType>
            <xs:sequence>
              <xs:element name="memoryCard" type="xs:string" maxOccurs="unbounded">
                <xs:annotation>
                  <xs:documentation>Refers to whether a phone has a memory card within it during capture. Typical memory cards are SD cards.</xs:documentation>
                </xs:annotation>
              </xs:element>
            </xs:sequence>
          </xs:complexType>
        </xs:element>
        <xs:element name="greetingMessage" type="xs:string" minOccurs="0">
          <xs:annotation>
            <xs:documentation>Refers to a possible message on a handset, which is displayed once the handset is turned on.</xs:documentation>
          </xs:annotation>
        </xs:element>
        <xs:element name="keypadLockCode" type="xs:string" minOccurs="0">
          <xs:annotation>
            <xs:documentation>The code to unlock a locked phone. Typically a 4 digit number.</xs:documentation>
          </xs:annotation>
        </xs:element>
        <xs:element name="bluetoothID" type="xs:string" minOccurs="0">
          <xs:annotation>
            <xs:documentation>The unique 48-bit address of the Bluetooth device.</xs:documentation>
          </xs:annotation>
        </xs:element>
      </xs:all>
    </xs:complexType>
Schema location | CellexReport.xsd Copy and paste this link to your file browser, clicking the link MAY open in the browser. Opening in an XML aware editor is best.

## This document has been approved for Public Release by the Office of the Director of National Intelligence. See Distribution Notice for details. Click Here