| ### Showing:
Annotations
Diagrams
Facets
Model
Properties
Source
Used by

Element ImageDetailsType / model

Namespace | urn:us:mil:ces:metadata:domex
Annotations | The image input equipment model name or number.
Diagram |
Type | string100
Properties |
content | simple
minOccurs | 0
Facets |
maxLength | 100 |
Source |
    <xs:element name="model" type="string100" minOccurs="0">
      <xs:annotation>
        <xs:documentation>The image input equipment model name or number.</xs:documentation>
      </xs:annotation>
    </xs:element>
Schema location | DOMEX.xsd Copy and paste this link to your file browser, clicking the link MAY open in the browser. Opening in an XML aware editor is best.

Element ImageDetailsType / make

Namespace | urn:us:mil:ces:metadata:domex
Annotations | The image input equipment manufacturer.
Diagram |
Type | string100
Properties |
content | simple
minOccurs | 0
Facets |
maxLength | 100 |
Source |
    <xs:element name="make" type="string100" minOccurs="0">
      <xs:annotation>
        <xs:documentation>The image input equipment manufacturer.</xs:documentation>
      </xs:annotation>
    </xs:element>
Schema location | DOMEX.xsd Copy and paste this link to your file browser, clicking the link MAY open in the browser. Opening in an XML aware editor is best.

Element ImageDetailsType / cameraSerialNumber

Namespace | urn:us:mil:ces:metadata:domex
Annotations | The image input equipment serial number.
Diagram |
Type | string100
Properties |
content | simple
minOccurs | 0
Facets |
maxLength | 100 |
Source |
    <xs:element name="cameraSerialNumber" type="string100" minOccurs="0">
      <xs:annotation>
        <xs:documentation>The image input equipment serial number.</xs:documentation>
      </xs:annotation>
    </xs:element>
Schema location | DOMEX.xsd Copy and paste this link to your file browser, clicking the link MAY open in the browser. Opening in an XML aware editor is best.

Element ImageDetailsType / dateTimeOriginal

Namespace | urn:us:mil:ces:metadata:domex
Annotations | The date and time of image creation.
Diagram |
Type | CombinedDateType
Properties |
content | simple
minOccurs | 0
Source |
    <xs:element name="dateTimeOriginal" type="irm:CombinedDateType" minOccurs="0">
      <xs:annotation>
        <xs:documentation>The date and time of image creation.</xs:documentation>
      </xs:annotation>
    </xs:element>
Schema location | DOMEX.xsd Copy and paste this link to your file browser, clicking the link MAY open in the browser. Opening in an XML aware editor is best.

Element ImageDetailsType / imageWidth

Namespace | urn:us:mil:ces:metadata:domex
Annotations | The number of columns of image data, equal to the number of pixels per row.
Diagram |
Type | xs:positiveInteger
Properties |
content | simple
minOccurs | 0
Source |
    <xs:element name="imageWidth" type="xs:positiveInteger" minOccurs="0">
      <xs:annotation>
        <xs:documentation>The number of columns of image data, equal to the number of pixels per row.</xs:documentation>
      </xs:annotation>
    </xs:element>
Schema location | DOMEX.xsd Copy and paste this link to your file browser, clicking the link MAY open in the browser. Opening in an XML aware editor is best.

Element ImageDetailsType / imageLength

Namespace | urn:us:mil:ces:metadata:domex
Annotations | The number of rows of image data.
Diagram |
Type | xs:positiveInteger
Properties |
content | simple
minOccurs | 0
Source |
    <xs:element name="imageLength" type="xs:positiveInteger" minOccurs="0">
      <xs:annotation>
        <xs:documentation>The number of rows of image data.</xs:documentation>
      </xs:annotation>
    </xs:element>
Schema location | DOMEX.xsd Copy and paste this link to your file browser, clicking the link MAY open in the browser. Opening in an XML aware editor is best.

Element ImageDetailsType / gpsCoordinates

Namespace | urn:us:mil:ces:metadata:domex
Annotations | The reported GPS coordinates expressed as degrees, minutes and seconds.
Diagram |
Type | PointType
Properties |
content | simple
minOccurs | 0
Source |
    <xs:element name="gpsCoordinates" type="tspi-core:PointType" minOccurs="0">
      <xs:annotation>
        <xs:documentation>The reported GPS coordinates expressed as degrees, minutes and seconds.</xs:documentation>
      </xs:annotation>
    </xs:element>
Schema location | DOMEX.xsd Copy and paste this link to your file browser, clicking the link MAY open in the browser. Opening in an XML aware editor is best.

Complex Type ImageDetailsType

Namespace | urn:us:mil:ces:metadata:domex
Annotations | Exchangeable Image File Format (EXIF) information. EXIF is the standard that specifies the formats to be used for images, sound and tags in digital still cameras and in other systems handling the image and sound files recorded by digital still cameras.
Diagram |
Used by |
Element | MediaFileType/exifImage
Model | model{0,1} , make{0,1} , cameraSerialNumber{0,1} , dateTimeOriginal{0,1} , imageWidth{0,1} , imageLength{0,1} , gpsCoordinates{0,1}
Children | cameraSerialNumber , dateTimeOriginal , gpsCoordinates , imageLength , imageWidth , make , model
Source |
    <xs:complexType name="ImageDetailsType">
      <xs:annotation>
        <xs:documentation>Exchangeable Image File Format (EXIF) information. EXIF is the standard that specifies the formats to be used for images, sound and tags in digital still cameras and in other systems handling the image and sound files recorded by digital still cameras.</xs:documentation>
      </xs:annotation>
      <xs:sequence>
        <xs:element name="model" type="string100" minOccurs="0">
          <xs:annotation>
            <xs:documentation>The image input equipment model name or number.</xs:documentation>
          </xs:annotation>
        </xs:element>
        <xs:element name="make" type="string100" minOccurs="0">
          <xs:annotation>
            <xs:documentation>The image input equipment manufacturer.</xs:documentation>
          </xs:annotation>
        </xs:element>
        <xs:element name="cameraSerialNumber" type="string100" minOccurs="0">
          <xs:annotation>
            <xs:documentation>The image input equipment serial number.</xs:documentation>
          </xs:annotation>
        </xs:element>
        <xs:element name="dateTimeOriginal" type="irm:CombinedDateType" minOccurs="0">
          <xs:annotation>
            <xs:documentation>The date and time of image creation.</xs:documentation>
          </xs:annotation>
        </xs:element>
        <xs:element name="imageWidth" type="xs:positiveInteger" minOccurs="0">
          <xs:annotation>
            <xs:documentation>The number of columns of image data, equal to the number of pixels per row.</xs:documentation>
          </xs:annotation>
        </xs:element>
        <xs:element name="imageLength" type="xs:positiveInteger" minOccurs="0">
          <xs:annotation>
            <xs:documentation>The number of rows of image data.</xs:documentation>
          </xs:annotation>
        </xs:element>
        <xs:element name="gpsCoordinates" type="tspi-core:PointType" minOccurs="0">
          <xs:annotation>
            <xs:documentation>The reported GPS coordinates expressed as degrees, minutes and seconds.</xs:documentation>
          </xs:annotation>
        </xs:element>
      </xs:sequence>
    </xs:complexType>
Schema location | DOMEX.xsd Copy and paste this link to your file browser, clicking the link MAY open in the browser. Opening in an XML aware editor is best.

## This document has been approved for Public Release by the Office of the Director of National Intelligence. See Distribution Notice for details. Click Here