| ### Showing:
Annotations
Diagrams
Model
Properties
Source
Used by

Element cr:ServiceTechnologyType / cr:MSISDN

Namespace | urn:CellexReport
Annotations | A number uniquely identifying a subscription in a Global System for Mobile Communications (GSM) or a Universal Mobile Telecommunications System (UMTS) mobile network. The abbreviation has several interpretations, the most common one being Mobile Subscriber Integrated Services Digital Network Number
Diagram |
Type | xs:string
Properties |
content | simple
minOccurs | 0
Source |
    <xs:element name="MSISDN" type="xs:string" minOccurs="0">
      <xs:annotation>
        <xs:documentation>A number uniquely identifying a subscription in a Global System for Mobile Communications (GSM) or a Universal Mobile Telecommunications System (UMTS) mobile network. The abbreviation has several interpretations, the most common one being Mobile Subscriber Integrated Services Digital Network Number</xs:documentation>
      </xs:annotation>
    </xs:element>
Schema location | CellexReport.xsd Copy and paste this link to your file browser, clicking the link MAY open in the browser. Opening in an XML aware editor is best.

Element cr:ServiceTechnologyType / cr:IMSI

Namespace | urn:CellexReport
Annotations | An International Mobile Subscriber Identity or IMSI is a unique identification associated with all GSM and UMTS network mobile phone users. It is stored as a 64-bit field in the SIM inside the phone and is sent by the phone to the network. It is also used for acquiring other details of the mobile in the Home Location Register (HLR) or as locally copied in the Visitor Location Register. To prevent eavesdroppers identifying and tracking the subscriber on the radio interface, the IMSI is sent as rarely as possible and a randomly-generated TMSI is sent instead.
Diagram |
Type | xs:string
Properties |
content | simple
minOccurs | 0
Source |
    <xs:element name="IMSI" type="xs:string" minOccurs="0">
      <xs:annotation>
        <xs:documentation>An International Mobile Subscriber Identity or IMSI is a unique identification associated with all GSM and UMTS network mobile phone users. It is stored as a 64-bit field in the SIM inside the phone and is sent by the phone to the network. It is also used for acquiring other details of the mobile in the Home Location Register (HLR) or as locally copied in the Visitor Location Register. To prevent eavesdroppers identifying and tracking the subscriber on the radio interface, the IMSI is sent as rarely as possible and a randomly-generated TMSI is sent instead.</xs:documentation>
      </xs:annotation>
    </xs:element>
Schema location | CellexReport.xsd Copy and paste this link to your file browser, clicking the link MAY open in the browser. Opening in an XML aware editor is best.

Element cr:ServiceTechnologyType / cr:TMSI

Namespace | urn:CellexReport
Annotations | The "Temporary Mobile Subscriber Identity" (TMSI) is the identity that is most commonly sent between the mobile and the network. TMSI is randomly assigned by the VLR to every mobile in the area, the moment it is switched on. The number is local to a location area, and so it has to be updated each time the mobile moves to a new geographical area.
Diagram |
Type | xs:string
Properties |
content | simple
minOccurs | 0
Source |
    <xs:element name="TMSI" type="xs:string" minOccurs="0">
      <xs:annotation>
        <xs:documentation>The "Temporary Mobile Subscriber Identity" (TMSI) is the identity that is most commonly sent between the mobile and the network. TMSI is randomly assigned by the VLR to every mobile in the area, the moment it is switched on. The number is local to a location area, and so it has to be updated each time the mobile moves to a new geographical area.</xs:documentation>
      </xs:annotation>
    </xs:element>
Schema location | CellexReport.xsd Copy and paste this link to your file browser, clicking the link MAY open in the browser. Opening in an XML aware editor is best.

Element cr:ServiceTechnologyType / cr:MMC

Namespace | urn:CellexReport
Annotations | Multi Media Card
Diagram |
Type | xs:string
Properties |
content | simple
minOccurs | 0
Source |
    <xs:element name="MMC" type="xs:string" minOccurs="0">
      <xs:annotation>
        <xs:documentation>Multi Media Card</xs:documentation>
      </xs:annotation>
    </xs:element>
Schema location | CellexReport.xsd Copy and paste this link to your file browser, clicking the link MAY open in the browser. Opening in an XML aware editor is best.

Element cr:ServiceTechnologyType / cr:MNC

Namespace | urn:CellexReport
Annotations | Is used in combination with a Mobile Country Code (MCC) (also known as a "MCC / MNC tuple") to uniquely identify a mobile phone operator/carrier using the GSM/LTE, CDMA, iDEN, TETRA and UMTS public land mobile networks and some satellite mobile networks. The ITU-T Recommendation E.212 defines mobile country codes.
Diagram |
Type | xs:string
Properties |
content | simple
minOccurs | 0
Source |
    <xs:element name="MNC" type="xs:string" minOccurs="0">
      <xs:annotation>
        <xs:documentation>Is used in combination with a Mobile Country Code (MCC) (also known as a "MCC / MNC tuple") to uniquely identify a mobile phone operator/carrier using the GSM/LTE, CDMA, iDEN, TETRA and UMTS public land mobile networks and some satellite mobile networks. The ITU-T Recommendation E.212 defines mobile country codes.</xs:documentation>
      </xs:annotation>
    </xs:element>
Schema location | CellexReport.xsd Copy and paste this link to your file browser, clicking the link MAY open in the browser. Opening in an XML aware editor is best.

Element cr:ServiceTechnologyType / cr:LAC

Namespace | urn:CellexReport
Annotations | Location Area Code
Diagram |
Type | xs:string
Properties |
content | simple
minOccurs | 0
Source |
    <xs:element name="LAC" type="xs:string" minOccurs="0">
      <xs:annotation>
        <xs:documentation>Location Area Code</xs:documentation>
      </xs:annotation>
    </xs:element>
Schema location | CellexReport.xsd Copy and paste this link to your file browser, clicking the link MAY open in the browser. Opening in an XML aware editor is best.

Element cr:ServiceTechnologyType / cr:ICCID

Namespace | urn:CellexReport
Annotations | Integrated circuit card identifier (ICCID). Each SIM is internationally identified by its ICCID. ICCIDs are stored in the SIM cards and are also engraved or printed on the SIM card body during a process called personalization. The ICCID is defined by the ITU-T recommendation E.118. According to E.118 the number is up to 19 digits long including a single check digit calculated using the Luhn algorithm. However, the GSM Phase 1 defined the ICC-ID length as 10 octets with operator-specific structure.
Diagram |
Type | xs:string
Properties |
content | simple
minOccurs | 0
Source |
    <xs:element name="ICCID" type="xs:string" minOccurs="0">
      <xs:annotation>
        <xs:documentation>Integrated circuit card identifier (ICCID). Each SIM is internationally identified by its ICCID. ICCIDs are stored in the SIM cards and are also engraved or printed on the SIM card body during a process called personalization. The ICCID is defined by the ITU-T recommendation E.118. According to E.118 the number is up to 19 digits long including a single check digit calculated using the Luhn algorithm. However, the GSM Phase 1 defined the ICC-ID length as 10 octets with operator-specific structure.</xs:documentation>
      </xs:annotation>
    </xs:element>
Schema location | CellexReport.xsd Copy and paste this link to your file browser, clicking the link MAY open in the browser. Opening in an XML aware editor is best.

Element cr:ServiceTechnologyType / cr:SimCardType

Namespace | urn:CellexReport
Annotations | A subscriber identity module (SIM) on a removable SIM card securely stores the service subscriber key (IMSI) used to identify a subscriber on mobile telephone devices (such as mobile phones and computers). The SIM card allows users to change phones by simply removing the SIM card from one mobile phone and inserting it into another mobile phone or broadband telephony device.
Diagram |
Type | xs:string
Properties |
content | simple
minOccurs | 0
Source |
    <xs:element name="SimCardType" type="xs:string" minOccurs="0">
      <xs:annotation>
        <xs:documentation>A subscriber identity module (SIM) on a removable SIM card securely stores the service subscriber key (IMSI) used to identify a subscriber on mobile telephone devices (such as mobile phones and computers). The SIM card allows users to change phones by simply removing the SIM card from one mobile phone and inserting it into another mobile phone or broadband telephony device.</xs:documentation>
      </xs:annotation>
    </xs:element>
Schema location | CellexReport.xsd Copy and paste this link to your file browser, clicking the link MAY open in the browser. Opening in an XML aware editor is best.

Element cr:ServiceTechnologyType / cr:ESN

Namespace | urn:CellexReport
Annotations | An electronic serial number (ESN) is the unique identification number embedded or inscribed on the microchip in a wireless phone by the manufacturer. Each time a call is placed, the ESN is automatically transmitted to the base station so the wireless carrier's mobile switching office check the call's validity. the ESN cannot easily be altered in the field. The ESN differs from the mobile identification number (MIN) which is the wireless carrier's identifier for a phone in the network. MINs and ESNs can be electronically checked to help prevent fraud. ESNs are mainly used with AMPS, TDMA and CDMA phones in the United States, compared to International Mobile Equipment Identity (IMEI) numbers used by all GSM phones.
Diagram |
Type | xs:string
Properties |
content | simple
minOccurs | 0
Source |
    <xs:element name="ESN" type="xs:string" minOccurs="0">
      <xs:annotation>
        <xs:documentation>An electronic serial number (ESN) is the unique identification number embedded or inscribed on the microchip in a wireless phone by the manufacturer. Each time a call is placed, the ESN is automatically transmitted to the base station so the wireless carrier's mobile switching office check the call's validity. the ESN cannot easily be altered in the field. The ESN differs from the mobile identification number (MIN) which is the wireless carrier's identifier for a phone in the network. MINs and ESNs can be electronically checked to help prevent fraud. ESNs are mainly used with AMPS, TDMA and CDMA phones in the United States, compared to International Mobile Equipment Identity (IMEI) numbers used by all GSM phones.</xs:documentation>
      </xs:annotation>
    </xs:element>
Schema location | CellexReport.xsd Copy and paste this link to your file browser, clicking the link MAY open in the browser. Opening in an XML aware editor is best.

Complex Type cr:ServiceTechnologyType

Namespace | urn:CellexReport
Diagram |
Used by |
Element | cr:CellexReportDataType/cr:serviceTechnologyInfo
Model | ALL( cr:MSISDN{0,1} cr:IMSI{0,1} cr:TMSI{0,1} cr:MMC{0,1} cr:MNC{0,1} cr:LAC{0,1} cr:ICCID{0,1} cr:SimCardType{0,1} cr:ESN{0,1} )
Children | cr:ESN , cr:ICCID , cr:IMSI , cr:LAC , cr:MMC , cr:MNC , cr:MSISDN , cr:SimCardType , cr:TMSI
Source |
    <xs:complexType name="ServiceTechnologyType">
      <xs:all>
        <xs:element name="MSISDN" type="xs:string" minOccurs="0">
          <xs:annotation>
            <xs:documentation>A number uniquely identifying a subscription in a Global System for Mobile Communications (GSM) or a Universal Mobile Telecommunications System (UMTS) mobile network. The abbreviation has several interpretations, the most common one being Mobile Subscriber Integrated Services Digital Network Number</xs:documentation>
          </xs:annotation>
        </xs:element>
        <xs:element name="IMSI" type="xs:string" minOccurs="0">
          <xs:annotation>
            <xs:documentation>An International Mobile Subscriber Identity or IMSI is a unique identification associated with all GSM and UMTS network mobile phone users. It is stored as a 64-bit field in the SIM inside the phone and is sent by the phone to the network. It is also used for acquiring other details of the mobile in the Home Location Register (HLR) or as locally copied in the Visitor Location Register. To prevent eavesdroppers identifying and tracking the subscriber on the radio interface, the IMSI is sent as rarely as possible and a randomly-generated TMSI is sent instead.</xs:documentation>
          </xs:annotation>
        </xs:element>
        <xs:element name="TMSI" type="xs:string" minOccurs="0">
          <xs:annotation>
            <xs:documentation>The "Temporary Mobile Subscriber Identity" (TMSI) is the identity that is most commonly sent between the mobile and the network. TMSI is randomly assigned by the VLR to every mobile in the area, the moment it is switched on. The number is local to a location area, and so it has to be updated each time the mobile moves to a new geographical area.</xs:documentation>
          </xs:annotation>
        </xs:element>
        <xs:element name="MMC" type="xs:string" minOccurs="0">
          <xs:annotation>
            <xs:documentation>Multi Media Card</xs:documentation>
          </xs:annotation>
        </xs:element>
        <xs:element name="MNC" type="xs:string" minOccurs="0">
          <xs:annotation>
            <xs:documentation>Is used in combination with a Mobile Country Code (MCC) (also known as a "MCC / MNC tuple") to uniquely identify a mobile phone operator/carrier using the GSM/LTE, CDMA, iDEN, TETRA and UMTS public land mobile networks and some satellite mobile networks. The ITU-T Recommendation E.212 defines mobile country codes.</xs:documentation>
          </xs:annotation>
        </xs:element>
        <xs:element name="LAC" type="xs:string" minOccurs="0">
          <xs:annotation>
            <xs:documentation>Location Area Code</xs:documentation>
          </xs:annotation>
        </xs:element>
        <xs:element name="ICCID" type="xs:string" minOccurs="0">
          <xs:annotation>
            <xs:documentation>Integrated circuit card identifier (ICCID). Each SIM is internationally identified by its ICCID. ICCIDs are stored in the SIM cards and are also engraved or printed on the SIM card body during a process called personalization. The ICCID is defined by the ITU-T recommendation E.118. According to E.118 the number is up to 19 digits long including a single check digit calculated using the Luhn algorithm. However, the GSM Phase 1 defined the ICC-ID length as 10 octets with operator-specific structure.</xs:documentation>
          </xs:annotation>
        </xs:element>
        <xs:element name="SimCardType" type="xs:string" minOccurs="0">
          <xs:annotation>
            <xs:documentation>A subscriber identity module (SIM) on a removable SIM card securely stores the service subscriber key (IMSI) used to identify a subscriber on mobile telephone devices (such as mobile phones and computers). The SIM card allows users to change phones by simply removing the SIM card from one mobile phone and inserting it into another mobile phone or broadband telephony device.</xs:documentation>
          </xs:annotation>
        </xs:element>
        <xs:element name="ESN" type="xs:string" minOccurs="0">
          <xs:annotation>
            <xs:documentation>An electronic serial number (ESN) is the unique identification number embedded or inscribed on the microchip in a wireless phone by the manufacturer. Each time a call is placed, the ESN is automatically transmitted to the base station so the wireless carrier's mobile switching office check the call's validity. the ESN cannot easily be altered in the field. The ESN differs from the mobile identification number (MIN) which is the wireless carrier's identifier for a phone in the network. MINs and ESNs can be electronically checked to help prevent fraud. ESNs are mainly used with AMPS, TDMA and CDMA phones in the United States, compared to International Mobile Equipment Identity (IMEI) numbers used by all GSM phones.</xs:documentation>
          </xs:annotation>
        </xs:element>
      </xs:all>
    </xs:complexType>
Schema location | CellexReport.xsd Copy and paste this link to your file browser, clicking the link MAY open in the browser. Opening in an XML aware editor is best.

## This document has been approved for Public Release by the Office of the Director of National Intelligence. See Distribution Notice for details. Click Here