| ### Showing:
Annotations
Diagrams
Instances
Model
Properties
Source
Used by

Element irm:postalAddress

Namespace | urn:us:gov:ic:irm
Annotations | ? ded:Definition: An element under geospatialCoverage that allows the specification of a place ("an identifiable part of any space") that is identified using (physical) addresses (e.g., postal address). Models a standalone postal address. ded:Obligation: (Conditional) ? geospatialCoverage must have at least one of geographicIdentifier, boundingGeometry, or postalAddress ded:Comment: TSPI encodes postalAddress as tspi:AbstractPhysicalAddress, permitting the use of substitution groups that are traced to the FGDC standard, including GeneralAddressClass, IntersectionAddress, LandmarkAddress, NumberedThoroughfareAddress, TwoNumberAddressRange, USPSGeneralDeliveryOffice, USPSPostalDeliveryBox, USPSPostalDeliveryRoute, and UnnumberedThoroughfareAddress. Details for the structure and encoding of postalAddress and its substitution groups are detailed in section 7 of the TSPI specification, which is used in conjunction with the FDGC standard.
Diagram |
Properties |
content | complex
Used by |
Complex Type | irm:PlaceType
Model | AbstractPhysicalAddress
Children | AbstractPhysicalAddress
Instance |
    <irm:postalAddress xmlns:irm="urn:us:gov:ic:irm">
      <AbstractPhysicalAddress>{1,1}</AbstractPhysicalAddress>
    </irm:postalAddress>
Source |
    <xsd:element name="postalAddress">
      <xsd:annotation>
        <xsd:documentation>&#x2028;
          <p xmlns="http://www.w3.org/1999/xhtml" ism:classification="U" ism:ownerProducer="USA" data-ded="ded:Definition">ded:Definition: An element under geospatialCoverage that allows the specification of a place ("an identifiable part of any space") that is identified using (physical) addresses (e.g., postal address). Models a standalone postal address.</p>
          <p xmlns="http://www.w3.org/1999/xhtml" ism:classification="U" ism:ownerProducer="USA" data-ded="ded:Obligation">ded:Obligation: (Conditional) ? geospatialCoverage must have at least one of geographicIdentifier, boundingGeometry, or postalAddress</p>
          <p xmlns="http://www.w3.org/1999/xhtml" ism:classification="U" ism:ownerProducer="USA" data-ded="ded:Comment">ded:Comment: TSPI encodes postalAddress as tspi:AbstractPhysicalAddress, permitting the use of substitution groups that are traced to the FGDC standard, including GeneralAddressClass, IntersectionAddress, LandmarkAddress, NumberedThoroughfareAddress, TwoNumberAddressRange, USPSGeneralDeliveryOffice, USPSPostalDeliveryBox, USPSPostalDeliveryRoute, and UnnumberedThoroughfareAddress. Details for the structure and encoding of postalAddress and its substitution groups are detailed in section 7 of the TSPI specification, which is used in conjunction with the FDGC standard.</p>
        </xsd:documentation>
      </xsd:annotation>
      <xsd:complexType>
        <xsd:group ref="irm:postalAddressGroup"/>
      </xsd:complexType>
    </xsd:element>
Schema location | IC-IRM.xsd Copy and paste this link to your file browser, clicking the link MAY open in the browser. Opening in an XML aware editor is best.

## This document has been approved for Public Release by the Office of the Director of National Intelligence. See Distribution Notice for details. Click Here