| ### Showing:
Annotations
Attributes
Diagrams
Properties
Source
Used by

Element irm:facilityIdentifier

Namespace | urn:us:gov:ic:irm
Annotations | ded:Definition: An element under geographicIdentifier that provides a code that uniquely identifies an installation or facility. ded:Obligation: (Conditional) a geographicIdentifier must have at least one of name, region, countryCode, subDivisionCode or facilityIdentifier.
Diagram |
Type | irm:FacilityIdentifierType
Properties |
content | complex
Used by |
Element | irm:geographicIdentifier
Attributes |
QName | Type | Use | Annotation
--- | --- | --- | ---
irm:beNumber | irm:simpleTokenType | required | ? ded:Definition: An attribute of facilityIdentifier that provides a DIA-specific identification number of a facility or installation according to a grid location system. (GMI:BE_NUMBER, 1.0) Uniquely identifies the installation of the facility. The BE_NUMBER is generated based on the value input for the COORD to determine the appropriate World Area Code (WAC), the system assigned record originator and a one-up-number. Pos. 1-4, World Area Code (WAC). Pos. 5, A hyphen, '-', or an 'E', in the fifth position indicates that position-6 will contain values 0-9. Alternately, the fifth position may contain the first of a two-character system assigned record originator code, position-6 will then contain the second character of the system assigned record originator code. Pos. 6, May contain the second character of the system assigned record originator code, the one-up-number series will then begin in position seven, and range from 0001-9909. If the one-up-number series begins in position 6, this position will contain the first of a five-position one-up-number, i.e., 00001-99999.Pos. 7-10, A one-up-number series. Depending on the content of position 5, the series may have begun in position 6 and have a range of 00001-99999. Or, have begun in position 7 and have a range from 0001-9999. ded:Obligation: (Conditional) Mandatory if facilityIdentifier is present. ded:Comment: If BE Number is supplied, no other elements are required to be supplied in the Geospatial Coverage category.
irm:osuffix | irm:simpleTokenType | optional | ? ded:Definition: An attribute of facilityIdentifier that provides a specific identification number for a facility located at the installation associated by the Facility BE Number. (GMI:OSUFFIX, 1.0) Uniquely identifies a facility or demographic area in conjunction with a BE_NUMBER. Pos. 1-2. SYSTEM ASSIGNED RECORD_ORIGINATOR. The organization creating the facility or demographic area. DIA installation records created prior to IDB generation of OSUFFIX contain DD.Pos. 3-5 A one-up number. ded:Obligation: (Optional) ded:Comment: Allowed only if BE Number is supplied.
Source |
    <xsd:element name="facilityIdentifier" type="irm:FacilityIdentifierType">
      <xsd:annotation>
        <xsd:documentation>
          <p xmlns="http://www.w3.org/1999/xhtml" ism:classification="U" ism:ownerProducer="USA" data-ded="ded:Definition">ded:Definition: An element under geographicIdentifier that provides a code that uniquely identifies an installation or facility.</p>
          <p xmlns="http://www.w3.org/1999/xhtml" ism:classification="U" ism:ownerProducer="USA" data-ded="ded:Obligation">ded:Obligation: (Conditional) a geographicIdentifier must have at least one of name, region, countryCode, subDivisionCode or facilityIdentifier.</p>
          <p xmlns="http://www.w3.org/1999/xhtml" ism:classification="U" ism:ownerProducer="USA" data-ded="ded:Comment"/>
        </xsd:documentation>
      </xsd:annotation>
    </xsd:element>
Schema location | IC-IRM.xsd Copy and paste this link to your file browser, clicking the link MAY open in the browser. Opening in an XML aware editor is best.

## This document has been approved for Public Release by the Office of the Director of National Intelligence. See Distribution Notice for details. Click Here